LOAFER SPECIFICATIONS AND EQUIPMENT LIST

**DIMENSIONS AND SPECIFICATIONS**

|  |  |
| --- | --- |
| **LOA** | 46'3" |
| **LWL** | 40'10" |
| **Beam** | 13'4" |
| **Draft** | 6'8" |
| **Displacement** | 33.300 lbs. |
| **Ballast** | 11.330 lbs. |
| **Sail Area**  | 1100 sq. ft. |
| **"I" measurement**  | 54' |
| **"P" measurement**  | 48' |
| **"J" measurement**  | 18'3" |
| **"E" measurement**  | 16' |
| **Power** | Westerbeke 82hp Diesel |
| **Fuel** | 150 gals. |
| **Water** | 200 gals. |

**HULL AND DECK**

* Hull and deck is hand laminated reinforced fiberglass Deck Airex cored
* The lead keel ballast is internally  fiberglass bonded in place
* Hull speed 8.65 knots
* Water tanks 4 stainless  800lt
* Fuel steel tanks 2, 600lts
* Berths Two cabin layout Three doubles one single
* Fridge and Freezer 12v new 2015 (both)
* pressure water hot and cold (9 gal hot water cyl )
* 9 lewmar winches 5 self-tailing
* Navtec Hydraulic vang and Backstay

**SAIL INVENTORY**

* Main new 2015 superdacron strong cruising sail (Willis sails)
* 2x genoa & staysails
* Gennaker in a sock, storm jib, Trysail

**ANCHORS  (4)**

* Bruce 60lb
* Danforth
* Fisherman
* CQR
* Stern anchor all set up with rode etc.
* Main anchor chain 90m 10mm hi test, various other warps ( long )
* Anchor Windlass  Nelson V1000

**ENGINE, GENERATOR, AND DRIVE TRAIN**

* MaxProp
* Dripless shaft seal new seals 2014 with 2 more spares
* Generator new just being installed Lombardini 4000 4kva
* Westerbeke Diesel 82hp approx 5000 hours.  Maintained to a high standard all oil changes 100 hours
* 130amp alternator
* Dual fuel filters
* Oil sump extraction pump,

**DINGHY AND OUTBOARD**

* Outboard 9.9 hp. in good condition
* Zodiac 2.7m tender
* Davits for dingy and lift for the out board.

**ELECTRICS**

* Battery charger inverter.  Magnum 100amp charger 3000w inverter new 2015
* Batteries all replaced 2015
	+ House: deep cycle gel. 540 amp hours
	+ Engine: start and generator batteries are 700 cold crank amps each.
* AC System is 110 volt (USA Power) throughout with step down transformer from 230v.
* DC system is 12v
* 3x 120watt solar panels on arch at rear

**INSTRUMENTS AND RADIOS**

* Furuno Radar
* Furuno GPS
* Compass Richie
* SSB Kenwood
* SCS Pactor modem
* VHF GME
* Auto pilot Robertson AP 11 and back up wheel mount unit
* Depth sounder is an Interphase twin scope (side-scan and forward scan SONAR)
* AIS is a Vesper Marine 850 Watchmate.

**SAFETY**

* Life Raft Avon 6 person
* 406 EPIRB
* Life sling
* Danbuoy
* Flares
* Life ring.

**GALLEY**

* LPG solenoid controlled from galley
* Oven 3 burner Force 10 new 2014

**MISCELLANEOUS**

* Covers full cockpit and other covers
* Stereo/cd player
* fire extinguishers (5)
* Fenders x 4
* 2x heads with manual toilets and showers
* 2x holding tanks
* Water makers (2)
	+ engine driven 120lt per hour membrane  replaced in 2012 high pressure pump 2014
	+ 2nd unit electric small survivor unit.
* There are extensive cruising spares and tools too numerous to mention for rigging, engine, and all systems on board; from bolt cutters to portable bilge pumps filters.

|  |  |
| --- | --- |
| **Vessel Name** | ***Loafer*** |
| **Type** | **KP46** |
| **Year of Manufacture** | **1983** |
| **Hull Number** | **8** |
| [**HIN**](http://www.kp44.org.dev/HIN.php) **(Hull Identification Number)** | **JKY460080383** |
| **Current Location** | **Marsden Cove Marina, New Zealand** |
| **Selling Price** | **USD 189,000** |
| **Owner** | **Hilary & Glennis Neilson** |
| **Contact (email)** | **hilary.glennis\_neilso@hotmail.com** |